|  |
| --- |
| Figure 1. Distribution of net height and spread for all nets used during the survey (numbered nets) and for all nets with measurement data since 2005. Circles show the average, box shows 25-75% range, thin line shows full range. Labels along the vertical axis show the number of hauls for each net. Colors show whether the average for a net fell within the 25-75% range for the full 2005-present data set. |

## Net number: 1

**Table** **:** Net deployment summary for net number 1 during 2023 survey.

| Field | Value |
| --- | --- |
| Gear | Poly Nor 'eastern |
| Net number | 1 |
| Year | 2023 |
| Survey | GOA |
| Vessel | 148 |
| Good hauls | 45 |
| Bad hauls | 2 |
| Avg. Height | 6.3 m |
| Avg. Spread | 16.9 m |
| Out of range |  |

**Table** **:** Trawl performance by haul for net number 1 during 2023 survey.

| Date | Vessel | Cruise | Haul | Performance |
| --- | --- | --- | --- | --- |
| 2023-06-06 | 148 | 202301 | 55 | Good performance |
| 2023-06-06 | 148 | 202301 | 56 | Good performance |
| 2023-06-06 | 148 | 202301 | 57 | Good performance |
| 2023-06-06 | 148 | 202301 | 58 | Good performance |
| 2023-06-07 | 148 | 202301 | 59 | Good performance |
| 2023-06-07 | 148 | 202301 | 60 | Good performance |
| 2023-06-07 | 148 | 202301 | 61 | Good performance |
| 2023-06-07 | 148 | 202301 | 62 | Good performance |
| 2023-06-07 | 148 | 202301 | 63 | Good performance |
| 2023-06-08 | 148 | 202301 | 64 | Good performance |
| 2023-06-08 | 148 | 202301 | 65 | Good performance |
| 2023-06-08 | 148 | 202301 | 66 | Good performance |
| 2023-06-08 | 148 | 202301 | 67 | Satisfactory performance, hauled back early due to hang(s) |
| 2023-06-08 | 148 | 202301 | 68 | Good performance |
| 2023-06-09 | 148 | 202301 | 69 | Good performance |
| 2023-06-09 | 148 | 202301 | 70 | Good performance |
| 2023-06-09 | 148 | 202301 | 71 | Good performance |
| 2023-06-09 | 148 | 202301 | 72 | Good performance |
| 2023-06-09 | 148 | 202301 | 73 | Good performance |
| 2023-06-10 | 148 | 202301 | 74 | Unsatisfactory performance, wing damaged |
| 2023-06-10 | 148 | 202301 | 75 | Satisfactory performance, footrope damaged |
| 2023-06-10 | 148 | 202301 | 76 | Good performance |
| 2023-06-11 | 148 | 202301 | 77 | Good performance |
| 2023-06-11 | 148 | 202301 | 78 | Good performance |
| 2023-06-11 | 148 | 202301 | 79 | Good performance |
| 2023-06-12 | 148 | 202301 | 80 | Good performance |
| 2023-06-12 | 148 | 202301 | 81 | Good performance |
| 2023-06-12 | 148 | 202301 | 82 | Good performance |
| 2023-06-12 | 148 | 202301 | 83 | Good performance |
| 2023-06-12 | 148 | 202301 | 84 | Good performance |
| 2023-06-13 | 148 | 202301 | 85 | Good performance |
| 2023-06-13 | 148 | 202301 | 86 | Good performance |
| 2023-06-13 | 148 | 202301 | 87 | Satisfactory performance, hauled back early due to hang(s) |
| 2023-06-13 | 148 | 202301 | 88 | Good performance |
| 2023-06-13 | 148 | 202301 | 89 | Good performance |
| 2023-06-13 | 148 | 202301 | 90 | Good performance |
| 2023-06-14 | 148 | 202301 | 91 | Good performance |
| 2023-06-14 | 148 | 202301 | 92 | Good performance |
| 2023-06-14 | 148 | 202301 | 93 | Satisfactory performance, hauled back early due to hang(s) |
| 2023-06-14 | 148 | 202301 | 94 | Good performance |
| 2023-06-14 | 148 | 202301 | 95 | Good performance |
| 2023-06-15 | 148 | 202301 | 96 | Good performance |
| 2023-06-15 | 148 | 202301 | 97 | Good performance |
| 2023-06-15 | 148 | 202301 | 98 | Good performance |
| 2023-06-16 | 148 | 202301 | 99 | Good performance |
| 2023-07-17 | 148 | 202301 | 228 | Good performance |
| 2023-07-18 | 148 | 202301 | 229 | Unsatisfactory performance, belly damaged |

## Net number: 3

**Table** **:** Net deployment summary for net number 3 during 2023 survey.

| Field | Value |
| --- | --- |
| Gear | Poly Nor 'eastern |
| Net number | 3 |
| Year | 2023 |
| Survey | GOA |
| Vessel | 148 |
| Good hauls | 44 |
| Bad hauls | 0 |
| Avg. Height | 7 m |
| Avg. Spread | 16.6 m |
| Out of range |  |

**Table** **:** Trawl performance by haul for net number 3 during 2023 survey.

| Date | Vessel | Cruise | Haul | Performance |
| --- | --- | --- | --- | --- |
| 2023-07-03 | 148 | 202301 | 171 | Good performance |
| 2023-07-03 | 148 | 202301 | 172 | Good performance |
| 2023-07-03 | 148 | 202301 | 173 | Good performance |
| 2023-07-03 | 148 | 202301 | 174 | Good performance |
| 2023-07-03 | 148 | 202301 | 175 | Good performance |
| 2023-07-04 | 148 | 202301 | 176 | Good performance |
| 2023-07-04 | 148 | 202301 | 177 | Good performance |
| 2023-07-04 | 148 | 202301 | 178 | Good performance |
| 2023-07-04 | 148 | 202301 | 179 | Good performance |
| 2023-07-04 | 148 | 202301 | 180 | Good performance |
| 2023-07-06 | 148 | 202301 | 181 | Good performance |
| 2023-07-06 | 148 | 202301 | 182 | Good performance |
| 2023-07-06 | 148 | 202301 | 183 | Good performance |
| 2023-07-06 | 148 | 202301 | 184 | Good performance |
| 2023-07-06 | 148 | 202301 | 185 | Good performance |
| 2023-07-07 | 148 | 202301 | 186 | Good performance |
| 2023-07-07 | 148 | 202301 | 187 | Good performance |
| 2023-07-07 | 148 | 202301 | 188 | Good performance |
| 2023-07-07 | 148 | 202301 | 189 | Good performance |
| 2023-07-07 | 148 | 202301 | 190 | Good performance |
| 2023-07-08 | 148 | 202301 | 191 | Satisfactory performance, minor hang(s) |
| 2023-07-08 | 148 | 202301 | 192 | Satisfactory performance, completed tow |
| 2023-07-08 | 148 | 202301 | 193 | Good performance |
| 2023-07-08 | 148 | 202301 | 194 | Good performance |
| 2023-07-08 | 148 | 202301 | 195 | Good performance |
| 2023-07-09 | 148 | 202301 | 196 | Good performance |
| 2023-07-09 | 148 | 202301 | 197 | Good performance |
| 2023-07-09 | 148 | 202301 | 198 | Good performance |
| 2023-07-09 | 148 | 202301 | 199 | Satisfactory performance, hauled back early due to hang(s) |
| 2023-07-09 | 148 | 202301 | 200 | Good performance |
| 2023-07-10 | 148 | 202301 | 201 | Good performance |
| 2023-07-10 | 148 | 202301 | 202 | Good performance |
| 2023-07-10 | 148 | 202301 | 203 | Good performance |
| 2023-07-10 | 148 | 202301 | 204 | Satisfactory performance, hauled back early due to hang(s) |
| 2023-07-10 | 148 | 202301 | 205 | Good performance |
| 2023-07-11 | 148 | 202301 | 206 | Good performance |
| 2023-07-11 | 148 | 202301 | 207 | Satisfactory performance, large fish catch affected net performance |
| 2023-07-11 | 148 | 202301 | 208 | Good performance |
| 2023-07-11 | 148 | 202301 | 209 | Good performance |
| 2023-07-12 | 148 | 202301 | 210 | Good performance |
| 2023-07-12 | 148 | 202301 | 211 | Good performance |
| 2023-07-12 | 148 | 202301 | 212 | Good performance |
| 2023-07-12 | 148 | 202301 | 213 | Satisfactory performance, caught debris or wreckage |
| 2023-07-13 | 148 | 202301 | 214 | Good performance |

## Net number: 5

**Table** **:** Net deployment summary for net number 5 during 2023 survey.

| Field | Value |
| --- | --- |
| Gear | Poly Nor 'eastern |
| Net number | 5 |
| Year | 2023 |
| Survey | GOA |
| Vessel | 176 |
| Good hauls | 40 |
| Bad hauls | 2 |
| Avg. Height | 6.8 m |
| Avg. Spread | 16 m |
| Out of range |  |

**Table** **:** Trawl performance by haul for net number 5 during 2023 survey.

| Date | Vessel | Cruise | Haul | Performance |
| --- | --- | --- | --- | --- |
| 2023-06-12 | 176 | 202301 | 86 | Good performance |
| 2023-06-12 | 176 | 202301 | 87 | Good performance |
| 2023-06-12 | 176 | 202301 | 88 | Good performance |
| 2023-06-12 | 176 | 202301 | 89 | Good performance |
| 2023-06-12 | 176 | 202301 | 90 | Satisfactory performance, minor hang(s) |
| 2023-06-13 | 176 | 202301 | 91 | Good performance |
| 2023-06-13 | 176 | 202301 | 92 | Good performance |
| 2023-06-13 | 176 | 202301 | 93 | Good performance |
| 2023-06-13 | 176 | 202301 | 94 | Good performance |
| 2023-06-13 | 176 | 202301 | 95 | Good performance |
| 2023-06-14 | 176 | 202301 | 96 | Good performance |
| 2023-06-14 | 176 | 202301 | 97 | Satisfactory performance, minor hang(s) |
| 2023-06-14 | 176 | 202301 | 98 | Good performance |
| 2023-06-14 | 176 | 202301 | 99 | Good performance |
| 2023-06-14 | 176 | 202301 | 100 | Good performance |
| 2023-06-14 | 176 | 202301 | 101 | Good performance |
| 2023-06-15 | 176 | 202301 | 102 | Good performance |
| 2023-06-15 | 176 | 202301 | 103 | Good performance |
| 2023-06-15 | 176 | 202301 | 104 | Good performance |
| 2023-06-15 | 176 | 202301 | 105 | Good performance |
| 2023-06-15 | 176 | 202301 | 106 | Good performance |
| 2023-06-15 | 176 | 202301 | 107 | Good performance |
| 2023-06-16 | 176 | 202301 | 108 | Good performance |
| 2023-06-16 | 176 | 202301 | 109 | Good performance |
| 2023-06-16 | 176 | 202301 | 110 | Good performance |
| 2023-06-16 | 176 | 202301 | 111 | Satisfactory performance, minor hang(s) |
| 2023-06-16 | 176 | 202301 | 112 | Good performance |
| 2023-06-17 | 176 | 202301 | 113 | Good performance |
| 2023-06-17 | 176 | 202301 | 114 | Satisfactory performance, large fish catch affected net performance |
| 2023-06-17 | 176 | 202301 | 115 | Good performance |
| 2023-06-17 | 176 | 202301 | 116 | Good performance |
| 2023-06-18 | 176 | 202301 | 117 | Good performance |
| 2023-06-18 | 176 | 202301 | 118 | Good performance |
| 2023-06-18 | 176 | 202301 | 119 | Good performance |
| 2023-06-18 | 176 | 202301 | 120 | Good performance |
| 2023-06-18 | 176 | 202301 | 121 | Good performance |
| 2023-06-18 | 176 | 202301 | 122 | Good performance |
| 2023-06-19 | 176 | 202301 | 123 | Good performance |
| 2023-06-19 | 176 | 202301 | 124 | Good performance |
| 2023-06-19 | 176 | 202301 | 125 | Unsatisfactory performance, Alaskan crab pot |
| 2023-06-19 | 176 | 202301 | 126 | Good performance |
| 2023-06-19 | 176 | 202301 | 127 | Unsatisfactory performance, major hang, stopped forward progress of vessel. |

## Net number: 7

**Table** **:** Net deployment summary for net number 7 during 2023 survey.

| Field | Value |
| --- | --- |
| Gear | Poly Nor 'eastern |
| Net number | 7 |
| Year | 2023 |
| Survey | GOA |
| Vessel | 176 |
| Good hauls | 52 |
| Bad hauls | 0 |
| Avg. Height | 6 m |
| Avg. Spread | 16.3 m |
| Out of range |  |

**Table** **:** Trawl performance by haul for net number 7 during 2023 survey.

| Date | Vessel | Cruise | Haul | Performance |
| --- | --- | --- | --- | --- |
| 2023-06-28 | 176 | 202301 | 155 | Good performance |
| 2023-06-28 | 176 | 202301 | 156 | Good performance |
| 2023-06-28 | 176 | 202301 | 157 | Good performance |
| 2023-06-29 | 176 | 202301 | 158 | Good performance |
| 2023-06-29 | 176 | 202301 | 159 | Good performance |
| 2023-06-29 | 176 | 202301 | 160 | Good performance |
| 2023-06-29 | 176 | 202301 | 161 | Good performance |
| 2023-06-29 | 176 | 202301 | 162 | Good performance |
| 2023-06-30 | 176 | 202301 | 163 | Good performance |
| 2023-06-30 | 176 | 202301 | 164 | Good performance |
| 2023-06-30 | 176 | 202301 | 165 | Good performance |
| 2023-06-30 | 176 | 202301 | 166 | Good performance |
| 2023-06-30 | 176 | 202301 | 167 | Good performance |
| 2023-07-01 | 176 | 202301 | 168 | Good performance |
| 2023-07-01 | 176 | 202301 | 169 | Good performance |
| 2023-07-01 | 176 | 202301 | 170 | Good performance |
| 2023-07-01 | 176 | 202301 | 171 | Good performance |
| 2023-07-03 | 176 | 202301 | 172 | Good performance |
| 2023-07-03 | 176 | 202301 | 173 | Good performance |
| 2023-07-03 | 176 | 202301 | 174 | Good performance |
| 2023-07-03 | 176 | 202301 | 175 | Good performance |
| 2023-07-04 | 176 | 202301 | 176 | Good performance |
| 2023-07-04 | 176 | 202301 | 177 | Good performance |
| 2023-07-04 | 176 | 202301 | 178 | Good performance |
| 2023-07-04 | 176 | 202301 | 179 | Good performance |
| 2023-07-04 | 176 | 202301 | 180 | Good performance |
| 2023-07-05 | 176 | 202301 | 181 | Good performance |
| 2023-07-05 | 176 | 202301 | 182 | Good performance |
| 2023-07-05 | 176 | 202301 | 183 | Good performance |
| 2023-07-05 | 176 | 202301 | 184 | Good performance |
| 2023-07-05 | 176 | 202301 | 185 | Good performance |
| 2023-07-06 | 176 | 202301 | 186 | Good performance |
| 2023-07-06 | 176 | 202301 | 187 | Good performance |
| 2023-07-06 | 176 | 202301 | 188 | Satisfactory performance, minor hang(s) |
| 2023-07-06 | 176 | 202301 | 189 | Good performance |
| 2023-07-06 | 176 | 202301 | 190 | Good performance |
| 2023-07-06 | 176 | 202301 | 191 | Good performance |
| 2023-07-07 | 176 | 202301 | 192 | Good performance |
| 2023-07-07 | 176 | 202301 | 193 | Good performance |
| 2023-07-07 | 176 | 202301 | 194 | Good performance |
| 2023-07-07 | 176 | 202301 | 195 | Good performance |
| 2023-07-07 | 176 | 202301 | 196 | Good performance |
| 2023-07-09 | 176 | 202301 | 197 | Good performance |
| 2023-07-09 | 176 | 202301 | 198 | Good performance |
| 2023-07-09 | 176 | 202301 | 199 | Good performance |
| 2023-07-10 | 176 | 202301 | 200 | Good performance |
| 2023-07-10 | 176 | 202301 | 201 | Good performance |
| 2023-07-10 | 176 | 202301 | 202 | Good performance |
| 2023-07-10 | 176 | 202301 | 203 | Good performance |
| 2023-07-11 | 176 | 202301 | 204 | Good performance |
| 2023-07-11 | 176 | 202301 | 205 | Good performance |
| 2023-07-11 | 176 | 202301 | 206 | Good performance |

## Net number: 13

**Table** **:** Net deployment summary for net number 13 during 2023 survey.

| Field | Value |
| --- | --- |
| Gear | Poly Nor 'eastern |
| Net number | 13 |
| Year | 2023 |
| Survey | GOA |
| Vessel | 148 |
| Good hauls | 47 |
| Bad hauls | 8 |
| Avg. Height | 6.5 m |
| Avg. Spread | 16.7 m |
| Out of range |  |

**Table** **:** Trawl performance by haul for net number 13 during 2023 survey.

| Date | Vessel | Cruise | Haul | Performance |
| --- | --- | --- | --- | --- |
| 2023-05-24 | 148 | 202301 | 7 | Good performance |
| 2023-05-24 | 148 | 202301 | 8 | Unsatisfactory performance, Alaskan crab pot |
| 2023-05-24 | 148 | 202301 | 9 | Good performance |
| 2023-05-24 | 148 | 202301 | 10 | Satisfactory performance, Alaskan crab pot |
| 2023-05-24 | 148 | 202301 | 11 | Unsatisfactory performance, belly damaged |
| 2023-05-25 | 148 | 202301 | 12 | Good performance |
| 2023-05-25 | 148 | 202301 | 13 | Good performance |
| 2023-05-26 | 148 | 202301 | 14 | Good performance |
| 2023-05-26 | 148 | 202301 | 15 | Good performance |
| 2023-05-26 | 148 | 202301 | 16 | Unsatisfactory performance, belly damaged |
| 2023-05-27 | 148 | 202301 | 19 | Good performance |
| 2023-05-27 | 148 | 202301 | 20 | Good performance |
| 2023-05-27 | 148 | 202301 | 21 | Good performance |
| 2023-05-27 | 148 | 202301 | 22 | Good performance |
| 2023-05-29 | 148 | 202301 | 23 | Good performance |
| 2023-05-29 | 148 | 202301 | 24 | Good performance |
| 2023-05-29 | 148 | 202301 | 25 | Good performance |
| 2023-05-30 | 148 | 202301 | 26 | Good performance |
| 2023-05-30 | 148 | 202301 | 27 | Unsatisfactory performance, Alaskan crab pot |
| 2023-05-30 | 148 | 202301 | 29 | Good performance |
| 2023-05-30 | 148 | 202301 | 30 | Unsatisfactory performance, net improperly configured, unspecified reason |
| 2023-05-30 | 148 | 202301 | 31 | Good performance |
| 2023-05-31 | 148 | 202301 | 32 | Good performance |
| 2023-05-31 | 148 | 202301 | 33 | Good performance |
| 2023-05-31 | 148 | 202301 | 34 | Unsatisfactory performance, hung up |
| 2023-05-31 | 148 | 202301 | 35 | Good performance |
| 2023-05-31 | 148 | 202301 | 36 | Good performance |
| 2023-05-31 | 148 | 202301 | 37 | Good performance |
| 2023-06-01 | 148 | 202301 | 38 | Good performance |
| 2023-06-01 | 148 | 202301 | 39 | Good performance |
| 2023-06-01 | 148 | 202301 | 40 | Unsatisfactory performance, hauled back early due to hang(s) |
| 2023-06-01 | 148 | 202301 | 41 | Good performance |
| 2023-06-01 | 148 | 202301 | 42 | Satisfactory performance, wing damaged |
| 2023-06-02 | 148 | 202301 | 43 | Good performance |
| 2023-06-02 | 148 | 202301 | 44 | Good performance |
| 2023-06-02 | 148 | 202301 | 45 | Good performance |
| 2023-06-02 | 148 | 202301 | 46 | Good performance |
| 2023-06-03 | 148 | 202301 | 47 | Good performance |
| 2023-06-03 | 148 | 202301 | 48 | Good performance |
| 2023-06-03 | 148 | 202301 | 49 | Good performance |
| 2023-06-03 | 148 | 202301 | 50 | Good performance |
| 2023-06-03 | 148 | 202301 | 51 | Good performance |
| 2023-06-04 | 148 | 202301 | 52 | Good performance |
| 2023-06-04 | 148 | 202301 | 53 | Good performance |
| 2023-06-04 | 148 | 202301 | 54 | Good performance |
| 2023-07-18 | 148 | 202301 | 230 | Good performance |
| 2023-07-18 | 148 | 202301 | 231 | Good performance |
| 2023-07-18 | 148 | 202301 | 232 | Unsatisfactory performance, hauled back early due to hang(s) |
| 2023-07-18 | 148 | 202301 | 233 | Good performance |
| 2023-07-18 | 148 | 202301 | 234 | Good performance |
| 2023-07-19 | 148 | 202301 | 235 | Good performance |
| 2023-07-19 | 148 | 202301 | 236 | Good performance |
| 2023-07-19 | 148 | 202301 | 237 | Good performance |
| 2023-07-19 | 148 | 202301 | 238 | Good performance |
| 2023-07-20 | 148 | 202301 | 239 | Good performance |

## Net number: 14

**Table** **:** Net deployment summary for net number 14 during 2023 survey.

| Field | Value |
| --- | --- |
| Gear | Poly Nor 'eastern |
| Net number | 14 |
| Year | 2023 |
| Survey | GOA |
| Vessel | 148 |
| Good hauls | 50 |
| Bad hauls | 0 |
| Avg. Height | 6.6 m |
| Avg. Spread | 16.5 m |
| Out of range |  |

**Table** **:** Trawl performance by haul for net number 14 during 2023 survey.

| Date | Vessel | Cruise | Haul | Performance |
| --- | --- | --- | --- | --- |
| 2023-06-20 | 148 | 202301 | 121 | Good performance |
| 2023-06-21 | 148 | 202301 | 122 | Good performance |
| 2023-06-21 | 148 | 202301 | 123 | Satisfactory performance, hauled back early due to hang(s) |
| 2023-06-21 | 148 | 202301 | 124 | Good performance |
| 2023-06-21 | 148 | 202301 | 125 | Good performance |
| 2023-06-21 | 148 | 202301 | 126 | Good performance |
| 2023-06-21 | 148 | 202301 | 127 | Good performance |
| 2023-06-22 | 148 | 202301 | 128 | Good performance |
| 2023-06-22 | 148 | 202301 | 129 | Good performance |
| 2023-06-22 | 148 | 202301 | 130 | Good performance |
| 2023-06-22 | 148 | 202301 | 131 | Good performance |
| 2023-06-23 | 148 | 202301 | 132 | Good performance |
| 2023-06-23 | 148 | 202301 | 133 | Good performance |
| 2023-06-23 | 148 | 202301 | 134 | Good performance |
| 2023-06-23 | 148 | 202301 | 135 | Good performance |
| 2023-06-23 | 148 | 202301 | 136 | Good performance |
| 2023-06-23 | 148 | 202301 | 137 | Satisfactory performance, hauled back early due to hang(s) |
| 2023-06-26 | 148 | 202301 | 138 | Good performance |
| 2023-06-26 | 148 | 202301 | 139 | Good performance |
| 2023-06-26 | 148 | 202301 | 140 | Good performance |
| 2023-06-26 | 148 | 202301 | 141 | Good performance |
| 2023-06-27 | 148 | 202301 | 142 | Good performance |
| 2023-06-27 | 148 | 202301 | 143 | Good performance |
| 2023-06-27 | 148 | 202301 | 144 | Good performance |
| 2023-06-27 | 148 | 202301 | 145 | Good performance |
| 2023-06-27 | 148 | 202301 | 146 | Good performance |
| 2023-06-28 | 148 | 202301 | 147 | Good performance |
| 2023-06-28 | 148 | 202301 | 148 | Good performance |
| 2023-06-28 | 148 | 202301 | 149 | Good performance |
| 2023-06-28 | 148 | 202301 | 150 | Good performance |
| 2023-06-28 | 148 | 202301 | 151 | Good performance |
| 2023-06-29 | 148 | 202301 | 152 | Good performance |
| 2023-06-29 | 148 | 202301 | 153 | Good performance |
| 2023-06-29 | 148 | 202301 | 154 | Good performance |
| 2023-06-29 | 148 | 202301 | 155 | Satisfactory performance, large fish catch affected net performance |
| 2023-06-29 | 148 | 202301 | 156 | Good performance |
| 2023-06-30 | 148 | 202301 | 157 | Good performance |
| 2023-06-30 | 148 | 202301 | 158 | Good performance |
| 2023-06-30 | 148 | 202301 | 159 | Good performance |
| 2023-06-30 | 148 | 202301 | 160 | Good performance |
| 2023-06-30 | 148 | 202301 | 161 | Good performance |
| 2023-07-01 | 148 | 202301 | 162 | Good performance |
| 2023-07-01 | 148 | 202301 | 163 | Good performance |
| 2023-07-01 | 148 | 202301 | 164 | Good performance |
| 2023-07-01 | 148 | 202301 | 165 | Good performance |
| 2023-07-01 | 148 | 202301 | 166 | Satisfactory performance, large fish catch affected net performance |
| 2023-07-02 | 148 | 202301 | 167 | Good performance |
| 2023-07-02 | 148 | 202301 | 168 | Satisfactory performance, caught pot, unspecified type |
| 2023-07-02 | 148 | 202301 | 169 | Good performance |
| 2023-07-02 | 148 | 202301 | 170 | Satisfactory performance, large fish catch affected net performance |

## Net number: 15

**Table** **:** Net deployment summary for net number 15 during 2023 survey.

| Field | Value |
| --- | --- |
| Gear | Poly Nor 'eastern |
| Net number | 15 |
| Year | 2023 |
| Survey | GOA |
| Vessel | 176 |
| Good hauls | 17 |
| Bad hauls | 0 |
| Avg. Height | 5.9 m |
| Avg. Spread | 16.3 m |
| Out of range |  |

**Table** **:** Trawl performance by haul for net number 15 during 2023 survey.

| Date | Vessel | Cruise | Haul | Performance |
| --- | --- | --- | --- | --- |
| 2023-07-30 | 176 | 202301 | 260 | Good performance |
| 2023-07-30 | 176 | 202301 | 261 | Good performance |
| 2023-07-30 | 176 | 202301 | 262 | Good performance |
| 2023-07-31 | 176 | 202301 | 263 | Good performance |
| 2023-07-31 | 176 | 202301 | 264 | Good performance |
| 2023-07-31 | 176 | 202301 | 265 | Good performance |
| 2023-08-01 | 176 | 202301 | 266 | Good performance |
| 2023-08-01 | 176 | 202301 | 267 | Good performance |
| 2023-08-01 | 176 | 202301 | 268 | Good performance |
| 2023-08-02 | 176 | 202301 | 269 | Good performance |
| 2023-08-02 | 176 | 202301 | 271 | Good performance |
| 2023-08-03 | 176 | 202301 | 272 | Good performance |
| 2023-08-03 | 176 | 202301 | 273 | Good performance |
| 2023-08-03 | 176 | 202301 | 274 | Good performance |
| 2023-08-03 | 176 | 202301 | 275 | Good performance |
| 2023-08-04 | 176 | 202301 | 276 | Good performance |
| 2023-08-04 | 176 | 202301 | 277 | Good performance |

## Net number: 17

**Table** **:** Net deployment summary for net number 17 during 2023 survey.

| Field | Value |
| --- | --- |
| Gear | Poly Nor 'eastern |
| Net number | 17 |
| Year | 2023 |
| Survey | GOA |
| Vessel | 148 |
| Good hauls | 13 |
| Bad hauls | 2 |
| Avg. Height | 6.6 m |
| Avg. Spread | 16.5 m |
| Out of range |  |

**Table** **:** Trawl performance by haul for net number 17 during 2023 survey.

| Date | Vessel | Cruise | Haul | Performance |
| --- | --- | --- | --- | --- |
| 2023-06-17 | 148 | 202301 | 100 | Good performance |
| 2023-06-17 | 148 | 202301 | 101 | Good performance |
| 2023-06-17 | 148 | 202301 | 102 | Good performance |
| 2023-06-17 | 148 | 202301 | 103 | Good performance |
| 2023-06-18 | 148 | 202301 | 104 | Unsatisfactory performance, wing damaged |
| 2023-06-18 | 148 | 202301 | 105 | Good performance |
| 2023-06-18 | 148 | 202301 | 106 | Good performance |
| 2023-06-18 | 148 | 202301 | 107 | Good performance |
| 2023-06-18 | 148 | 202301 | 108 | Good performance |
| 2023-06-18 | 148 | 202301 | 109 | Good performance |
| 2023-06-19 | 148 | 202301 | 110 | Good performance |
| 2023-06-19 | 148 | 202301 | 111 | Good performance |
| 2023-06-19 | 148 | 202301 | 112 | Good performance |
| 2023-06-19 | 148 | 202301 | 113 | Good performance |
| 2023-06-19 | 148 | 202301 | 114 | Unsatisfactory performance, net completely destroyed |

## Net number: 19

**Table** **:** Net deployment summary for net number 19 during 2023 survey.

| Field | Value |
| --- | --- |
| Gear | Poly Nor 'eastern |
| Net number | 19 |
| Year | 2023 |
| Survey | GOA |
| Vessel | 148 |
| Good hauls | 47 |
| Bad hauls | 1 |
| Avg. Height | 6.6 m |
| Avg. Spread | 17.1 m |
| Out of range |  |

**Table** **:** Trawl performance by haul for net number 19 during 2023 survey.

| Date | Vessel | Cruise | Haul | Performance |
| --- | --- | --- | --- | --- |
| 2023-05-26 | 148 | 202301 | 17 | Good performance |
| 2023-05-26 | 148 | 202301 | 18 | Good performance |
| 2023-05-30 | 148 | 202301 | 28 | Good performance |
| 2023-06-19 | 148 | 202301 | 115 | Good performance |
| 2023-06-19 | 148 | 202301 | 116 | Good performance |
| 2023-06-19 | 148 | 202301 | 117 | Good performance |
| 2023-06-20 | 148 | 202301 | 118 | Good performance |
| 2023-06-20 | 148 | 202301 | 119 | Good performance |
| 2023-06-20 | 148 | 202301 | 120 | Good performance |
| 2023-07-17 | 148 | 202301 | 227 | Good performance |
| 2023-07-20 | 148 | 202301 | 240 | Good performance |
| 2023-07-20 | 148 | 202301 | 241 | Good performance |
| 2023-07-20 | 148 | 202301 | 242 | Good performance |
| 2023-07-21 | 148 | 202301 | 243 | Good performance |
| 2023-07-21 | 148 | 202301 | 244 | Good performance |
| 2023-07-21 | 148 | 202301 | 245 | Satisfactory performance, wing damaged |
| 2023-07-21 | 148 | 202301 | 246 | Good performance |
| 2023-07-22 | 148 | 202301 | 247 | Good performance |
| 2023-07-22 | 148 | 202301 | 248 | Good performance |
| 2023-07-22 | 148 | 202301 | 249 | Unsatisfactory performance headrope/footrope tangled |
| 2023-07-22 | 148 | 202301 | 250 | Good performance |
| 2023-07-22 | 148 | 202301 | 251 | Good performance |
| 2023-07-23 | 148 | 202301 | 252 | Good performance |
| 2023-07-23 | 148 | 202301 | 253 | Good performance |
| 2023-07-23 | 148 | 202301 | 254 | Good performance |
| 2023-07-23 | 148 | 202301 | 255 | Good performance |
| 2023-07-25 | 148 | 202301 | 256 | Good performance |
| 2023-07-25 | 148 | 202301 | 257 | Satisfactory performance, hauled back early due to hang(s) |
| 2023-07-25 | 148 | 202301 | 258 | Good performance |
| 2023-07-26 | 148 | 202301 | 259 | Good performance |
| 2023-07-26 | 148 | 202301 | 260 | Good performance |
| 2023-07-26 | 148 | 202301 | 261 | Satisfactory performance, hauled back early due to hang(s) |
| 2023-07-26 | 148 | 202301 | 262 | Good performance |
| 2023-07-26 | 148 | 202301 | 263 | Good performance |
| 2023-07-26 | 148 | 202301 | 264 | Good performance |
| 2023-07-27 | 148 | 202301 | 266 | Good performance |
| 2023-07-27 | 148 | 202301 | 267 | Good performance |
| 2023-07-27 | 148 | 202301 | 268 | Good performance |
| 2023-07-28 | 148 | 202301 | 269 | Good performance |
| 2023-07-28 | 148 | 202301 | 270 | Good performance |
| 2023-07-28 | 148 | 202301 | 271 | Satisfactory performance, minor hang(s) |
| 2023-07-28 | 148 | 202301 | 272 | Good performance |
| 2023-07-29 | 148 | 202301 | 273 | Satisfactory performance, hauled back early due to hang(s) |
| 2023-07-29 | 148 | 202301 | 274 | Good performance |
| 2023-07-30 | 148 | 202301 | 275 | Good performance |
| 2023-07-30 | 148 | 202301 | 276 | Good performance |
| 2023-07-30 | 148 | 202301 | 277 | Good performance |
| 2023-07-30 | 148 | 202301 | 278 | Good performance |

## Net number: 21

**Table** **:** Net deployment summary for net number 21 during 2023 survey.

| Field | Value |
| --- | --- |
| Gear | Poly Nor 'eastern |
| Net number | 21 |
| Year | 2023 |
| Survey | GOA |
| Vessel | 176 |
| Good hauls | 36 |
| Bad hauls | 3 |
| Avg. Height | 6.5 m |
| Avg. Spread | 16 m |
| Out of range |  |

**Table** **:** Trawl performance by haul for net number 21 during 2023 survey.

| Date | Vessel | Cruise | Haul | Performance |
| --- | --- | --- | --- | --- |
| 2023-06-19 | 176 | 202301 | 128 | Good performance |
| 2023-06-21 | 176 | 202301 | 129 | Good performance |
| 2023-06-21 | 176 | 202301 | 130 | Good performance |
| 2023-06-21 | 176 | 202301 | 131 | Good performance |
| 2023-06-21 | 176 | 202301 | 132 | Satisfactory performance, hauled back early due to hang(s) |
| 2023-06-21 | 176 | 202301 | 133 | Satisfactory performance, minor hang(s) |
| 2023-06-21 | 176 | 202301 | 134 | Good performance |
| 2023-06-22 | 176 | 202301 | 135 | Good performance |
| 2023-06-22 | 176 | 202301 | 136 | Good performance |
| 2023-06-22 | 176 | 202301 | 137 | Good performance |
| 2023-06-22 | 176 | 202301 | 138 | Good performance |
| 2023-06-22 | 176 | 202301 | 139 | Good performance |
| 2023-06-23 | 176 | 202301 | 140 | Good performance |
| 2023-06-23 | 176 | 202301 | 141 | Good performance |
| 2023-06-23 | 176 | 202301 | 142 | Good performance |
| 2023-06-23 | 176 | 202301 | 143 | Good performance |
| 2023-06-23 | 176 | 202301 | 144 | Good performance |
| 2023-06-24 | 176 | 202301 | 145 | Good performance |
| 2023-06-24 | 176 | 202301 | 146 | Good performance |
| 2023-06-26 | 176 | 202301 | 147 | Good performance |
| 2023-06-27 | 176 | 202301 | 148 | Good performance |
| 2023-06-27 | 176 | 202301 | 149 | Good performance |
| 2023-06-27 | 176 | 202301 | 150 | Good performance |
| 2023-06-27 | 176 | 202301 | 151 | Good performance |
| 2023-06-28 | 176 | 202301 | 152 | Good performance |
| 2023-06-28 | 176 | 202301 | 153 | Satisfactory performance, minor hang(s) |
| 2023-06-28 | 176 | 202301 | 154 | Unsatisfactory performance, belly damaged |
| 2023-07-24 | 176 | 202301 | 247 | Good performance |
| 2023-07-24 | 176 | 202301 | 248 | Good performance |
| 2023-07-24 | 176 | 202301 | 249 | Good performance |
| 2023-07-26 | 176 | 202301 | 250 | Good performance |
| 2023-07-26 | 176 | 202301 | 251 | Unsatisfactory performance, hauled back early due to hang(s) |
| 2023-07-26 | 176 | 202301 | 252 | Good performance |
| 2023-07-26 | 176 | 202301 | 253 | Good performance |
| 2023-07-27 | 176 | 202301 | 254 | Good performance |
| 2023-07-28 | 176 | 202301 | 255 | Good performance |
| 2023-07-28 | 176 | 202301 | 257 | Good performance |
| 2023-07-29 | 176 | 202301 | 258 | Good performance |
| 2023-07-29 | 176 | 202301 | 259 | Unsatisfactory performance, belly damaged |

## Net number: 22

**Table** **:** Net deployment summary for net number 22 during 2023 survey.

| Field | Value |
| --- | --- |
| Gear | Poly Nor 'eastern |
| Net number | 22 |
| Year | 2023 |
| Survey | GOA |
| Vessel | 148 |
| Good hauls | 9 |
| Bad hauls | 3 |
| Avg. Height | 6 m |
| Avg. Spread | 17.4 m |
| Out of range |  |

**Table** **:** Trawl performance by haul for net number 22 during 2023 survey.

| Date | Vessel | Cruise | Haul | Performance |
| --- | --- | --- | --- | --- |
| 2023-07-15 | 148 | 202301 | 215 | Satisfactory performance, completed tow |
| 2023-07-15 | 148 | 202301 | 216 | Unsatisfactory performance, bridle damaged |
| 2023-07-15 | 148 | 202301 | 217 | Unsatisfactory performance, unspecified mechanical problems |
| 2023-07-15 | 148 | 202301 | 218 | Good performance |
| 2023-07-15 | 148 | 202301 | 219 | Good performance |
| 2023-07-15 | 148 | 202301 | 220 | Good performance |
| 2023-07-16 | 148 | 202301 | 221 | Good performance |
| 2023-07-16 | 148 | 202301 | 222 | Good performance |
| 2023-07-16 | 148 | 202301 | 223 | Good performance |
| 2023-07-16 | 148 | 202301 | 224 | Good performance |
| 2023-07-17 | 148 | 202301 | 225 | Good performance |
| 2023-07-17 | 148 | 202301 | 226 | Unsatisfactory performance, belly damaged |

## Net number: 23

**Table** **:** Net deployment summary for net number 23 during 2023 survey.

| Field | Value |
| --- | --- |
| Gear | Poly Nor 'eastern |
| Net number | 23 |
| Year | 2023 |
| Survey | GOA |
| Vessel | 176 |
| Good hauls | 45 |
| Bad hauls | 0 |
| Avg. Height | 6.3 m |
| Avg. Spread | 16.5 m |
| Out of range |  |

**Table** **:** Trawl performance by haul for net number 23 during 2023 survey.

| Date | Vessel | Cruise | Haul | Performance |
| --- | --- | --- | --- | --- |
| 2023-05-31 | 176 | 202301 | 41 | Good performance |
| 2023-05-31 | 176 | 202301 | 42 | Satisfactory performance, completed tow |
| 2023-05-31 | 176 | 202301 | 43 | Good performance |
| 2023-05-31 | 176 | 202301 | 44 | Good performance |
| 2023-06-01 | 176 | 202301 | 45 | Good performance |
| 2023-06-01 | 176 | 202301 | 46 | Good performance |
| 2023-06-01 | 176 | 202301 | 47 | Good performance |
| 2023-06-01 | 176 | 202301 | 48 | Good performance |
| 2023-06-01 | 176 | 202301 | 49 | Good performance |
| 2023-06-02 | 176 | 202301 | 50 | Good performance |
| 2023-06-02 | 176 | 202301 | 51 | Good performance |
| 2023-06-02 | 176 | 202301 | 52 | Good performance |
| 2023-06-02 | 176 | 202301 | 53 | Good performance |
| 2023-06-02 | 176 | 202301 | 54 | Good performance |
| 2023-06-03 | 176 | 202301 | 55 | Good performance |
| 2023-06-03 | 176 | 202301 | 56 | Good performance |
| 2023-06-03 | 176 | 202301 | 57 | Good performance |
| 2023-06-03 | 176 | 202301 | 58 | Good performance |
| 2023-06-04 | 176 | 202301 | 59 | Good performance |
| 2023-06-04 | 176 | 202301 | 60 | Good performance |
| 2023-06-04 | 176 | 202301 | 61 | Good performance |
| 2023-06-06 | 176 | 202301 | 62 | Good performance |
| 2023-06-06 | 176 | 202301 | 63 | Good performance |
| 2023-06-06 | 176 | 202301 | 64 | Good performance |
| 2023-06-06 | 176 | 202301 | 65 | Good performance |
| 2023-06-07 | 176 | 202301 | 66 | Good performance |
| 2023-06-07 | 176 | 202301 | 67 | Good performance |
| 2023-06-07 | 176 | 202301 | 68 | Good performance |
| 2023-06-07 | 176 | 202301 | 69 | Good performance |
| 2023-06-07 | 176 | 202301 | 70 | Good performance |
| 2023-06-08 | 176 | 202301 | 71 | Good performance |
| 2023-06-08 | 176 | 202301 | 72 | Good performance |
| 2023-06-08 | 176 | 202301 | 73 | Good performance |
| 2023-06-08 | 176 | 202301 | 74 | Good performance |
| 2023-06-08 | 176 | 202301 | 75 | Good performance |
| 2023-06-09 | 176 | 202301 | 76 | Satisfactory performance, hauled back early due to hang(s) |
| 2023-06-09 | 176 | 202301 | 77 | Good performance |
| 2023-06-09 | 176 | 202301 | 78 | Good performance |
| 2023-06-09 | 176 | 202301 | 79 | Good performance |
| 2023-06-10 | 176 | 202301 | 80 | Good performance |
| 2023-06-10 | 176 | 202301 | 81 | Good performance |
| 2023-06-10 | 176 | 202301 | 82 | Good performance |
| 2023-06-10 | 176 | 202301 | 83 | Good performance |
| 2023-06-10 | 176 | 202301 | 84 | Good performance |
| 2023-06-10 | 176 | 202301 | 85 | Good performance |

## Net number: 26

**Table** **:** Net deployment summary for net number 26 during 2023 survey.

| Field | Value |
| --- | --- |
| Gear | Poly Nor 'eastern |
| Net number | 26 |
| Year | 2023 |
| Survey | GOA |
| Vessel | 176 |
| Good hauls | 36 |
| Bad hauls | 1 |
| Avg. Height | 6.3 m |
| Avg. Spread | 16.6 m |
| Out of range |  |

**Table** **:** Trawl performance by haul for net number 26 during 2023 survey.

| Date | Vessel | Cruise | Haul | Performance |
| --- | --- | --- | --- | --- |
| 2023-05-21 | 176 | 202301 | 4 | Good performance |
| 2023-05-22 | 176 | 202301 | 5 | Good performance |
| 2023-05-22 | 176 | 202301 | 6 | Good performance |
| 2023-05-22 | 176 | 202301 | 7 | Good performance |
| 2023-05-23 | 176 | 202301 | 8 | Good performance |
| 2023-05-23 | 176 | 202301 | 9 | Good performance |
| 2023-05-23 | 176 | 202301 | 10 | Good performance |
| 2023-05-23 | 176 | 202301 | 11 | Good performance |
| 2023-05-23 | 176 | 202301 | 12 | Good performance |
| 2023-05-24 | 176 | 202301 | 13 | Good performance |
| 2023-05-24 | 176 | 202301 | 14 | Good performance |
| 2023-05-24 | 176 | 202301 | 15 | Good performance |
| 2023-05-24 | 176 | 202301 | 16 | Good performance |
| 2023-05-24 | 176 | 202301 | 17 | Good performance |
| 2023-05-25 | 176 | 202301 | 18 | Good performance |
| 2023-05-25 | 176 | 202301 | 19 | Good performance |
| 2023-05-25 | 176 | 202301 | 20 | Good performance |
| 2023-05-25 | 176 | 202301 | 21 | Good performance |
| 2023-05-26 | 176 | 202301 | 22 | Good performance |
| 2023-05-26 | 176 | 202301 | 23 | Good performance |
| 2023-05-26 | 176 | 202301 | 24 | Good performance |
| 2023-05-26 | 176 | 202301 | 25 | Good performance |
| 2023-05-27 | 176 | 202301 | 26 | Satisfactory performance, minor hang(s) |
| 2023-05-27 | 176 | 202301 | 27 | Good performance |
| 2023-05-27 | 176 | 202301 | 28 | Good performance |
| 2023-05-27 | 176 | 202301 | 29 | Good performance |
| 2023-05-28 | 176 | 202301 | 30 | Good performance |
| 2023-05-28 | 176 | 202301 | 31 | Good performance |
| 2023-05-28 | 176 | 202301 | 32 | Good performance |
| 2023-05-28 | 176 | 202301 | 33 | Good performance |
| 2023-05-28 | 176 | 202301 | 34 | Good performance |
| 2023-05-29 | 176 | 202301 | 35 | Good performance |
| 2023-05-29 | 176 | 202301 | 36 | Unsatisfactory performance, hung up |
| 2023-05-29 | 176 | 202301 | 37 | Good performance |
| 2023-05-29 | 176 | 202301 | 38 | Good performance |
| 2023-05-29 | 176 | 202301 | 39 | Good performance |
| 2023-05-29 | 176 | 202301 | 40 | Good performance |

## Net number: 28

**Table** **:** Net deployment summary for net number 28 during 2023 survey.

| Field | Value |
| --- | --- |
| Gear | Poly Nor 'eastern |
| Net number | 28 |
| Year | 2023 |
| Survey | GOA |
| Vessel | 176 |
| Good hauls | 37 |
| Bad hauls | 2 |
| Avg. Height | 6.5 m |
| Avg. Spread | 16.9 m |
| Out of range |  |

**Table** **:** Trawl performance by haul for net number 28 during 2023 survey.

| Date | Vessel | Cruise | Haul | Performance |
| --- | --- | --- | --- | --- |
| 2023-07-12 | 176 | 202301 | 207 | Good performance |
| 2023-07-12 | 176 | 202301 | 208 | Good performance |
| 2023-07-12 | 176 | 202301 | 209 | Good performance |
| 2023-07-13 | 176 | 202301 | 210 | Good performance |
| 2023-07-15 | 176 | 202301 | 211 | Good performance |
| 2023-07-15 | 176 | 202301 | 212 | Good performance |
| 2023-07-15 | 176 | 202301 | 213 | Good performance |
| 2023-07-16 | 176 | 202301 | 214 | Good performance |
| 2023-07-16 | 176 | 202301 | 215 | Good performance |
| 2023-07-16 | 176 | 202301 | 216 | Unsatisfactory performance, major hang, stopped forward progress of vessel. |
| 2023-07-17 | 176 | 202301 | 217 | Good performance |
| 2023-07-17 | 176 | 202301 | 218 | Good performance |
| 2023-07-17 | 176 | 202301 | 219 | Good performance |
| 2023-07-18 | 176 | 202301 | 220 | Good performance |
| 2023-07-18 | 176 | 202301 | 221 | Good performance |
| 2023-07-18 | 176 | 202301 | 222 | Good performance |
| 2023-07-18 | 176 | 202301 | 223 | Good performance |
| 2023-07-18 | 176 | 202301 | 224 | Good performance |
| 2023-07-19 | 176 | 202301 | 225 | Good performance |
| 2023-07-19 | 176 | 202301 | 226 | Good performance |
| 2023-07-19 | 176 | 202301 | 227 | Good performance |
| 2023-07-19 | 176 | 202301 | 228 | Good performance |
| 2023-07-20 | 176 | 202301 | 230 | Good performance |
| 2023-07-20 | 176 | 202301 | 231 | Good performance |
| 2023-07-20 | 176 | 202301 | 232 | Good performance |
| 2023-07-20 | 176 | 202301 | 233 | Good performance |
| 2023-07-20 | 176 | 202301 | 234 | Good performance |
| 2023-07-21 | 176 | 202301 | 235 | Good performance |
| 2023-07-21 | 176 | 202301 | 236 | Good performance |
| 2023-07-21 | 176 | 202301 | 237 | Good performance |
| 2023-07-21 | 176 | 202301 | 238 | Good performance |
| 2023-07-22 | 176 | 202301 | 239 | Good performance |
| 2023-07-22 | 176 | 202301 | 240 | Good performance |
| 2023-07-22 | 176 | 202301 | 241 | Good performance |
| 2023-07-22 | 176 | 202301 | 242 | Good performance |
| 2023-07-23 | 176 | 202301 | 243 | Good performance |
| 2023-07-23 | 176 | 202301 | 244 | Good performance |
| 2023-07-23 | 176 | 202301 | 245 | Good performance |
| 2023-07-24 | 176 | 202301 | 246 | Unsatisfactory performance, bridle damaged |

## Net number: 91

**Table** **:** Net deployment summary for net number 91 during 2023 survey.

| Field | Value |
| --- | --- |
| Gear | Poly Nor 'eastern |
| Net number | 91 |
| Year | 2023 |
| Survey | GOA |
| Vessel | 148 |
| Good hauls | 4 |
| Bad hauls | 0 |
| Avg. Height | 6.4 m |
| Avg. Spread | 16.3 m |
| Out of range |  |

**Table** **:** Trawl performance by haul for net number 91 during 2023 survey.

| Date | Vessel | Cruise | Haul | Performance |
| --- | --- | --- | --- | --- |
| 2023-05-23 | 148 | 202301 | 3 | Good performance |
| 2023-05-23 | 148 | 202301 | 4 | Good performance |
| 2023-05-23 | 148 | 202301 | 5 | Good performance |
| 2023-05-23 | 148 | 202301 | 6 | Good performance |